TITLE:   DC7 R1_v8.2 
FCM: NON-DROP FRAME
001  OY_HEAD_ A2    C        00:00:00:00 00:00:00:00 01:00:00:00 01:00:08:00 
* FROM CLIP NAME:  HEAD LEADER MONO 
* PATCH OY_HEAD_:  FROM SOURCE 1 TO RECORD 2 
* SOURCE FILE: OY_HEAD_LEADER.MOV
002  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:00:00:00 01:04:24:06 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
003  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:00:00:00 01:04:24:07 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
004  TC_R1_V6 A11   C        00:00:00:00 00:00:00:00 01:00:00:00 01:04:24:07 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* SOURCE FILE: TC R1 V6 TEMP2 ST BG.WAV
005  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:00:00:00 01:04:24:07 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
006  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:04:24:06 01:04:24:06 
006  TC_R1_V6 A     D    002 00:00:00:00 00:00:00:00 01:04:24:06 01:04:24:08 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* TO CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
007  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:04:24:07 01:04:42:08 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
008  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:04:24:07 01:04:45:16 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
009  TC_R1_V6 A11   C        00:00:00:00 00:00:00:00 01:04:24:07 01:04:45:19 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* SOURCE FILE: TC R1 V6 TEMP2 ST BG.WAV
010  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:04:24:08 01:04:35:19 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
011  TC_R1_V1 A     C        00:00:00:00 00:00:00:00 01:04:35:19 01:04:46:16 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 DX M.WAV 
* SOURCE FILE: TC R1 V1.2 TEMP1 DX M.WAV
012  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:04:42:08 01:04:42:08 
012  TC_R1_V6 A12   D    002 00:00:00:00 00:00:00:00 01:04:42:08 01:04:42:10 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* TO CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
013  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:04:42:10 01:04:46:23 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
014  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:04:45:16 01:04:47:00 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
015  TC_R1_V6 A11   C        00:00:00:00 00:00:00:00 01:04:45:19 01:04:45:19 
015  TC_R1_V6 A11   D    002 00:00:00:00 00:00:00:00 01:04:45:19 01:04:45:21 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* TO CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* SOURCE FILE: TC R1 V6 TEMP2 ST BG.WAV
016  TC_R1_V6 A11   C        00:00:00:00 00:00:00:00 01:04:45:21 01:04:46:23 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* SOURCE FILE: TC R1 V6 TEMP2 ST BG.WAV
017  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:04:46:16 01:05:47:12 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
018  TC_R1_V6 A11   C        00:00:00:00 00:00:00:00 01:04:46:23 01:04:46:23 
018  TC_R1_V6 A11   D    002 00:00:00:00 00:00:00:00 01:04:46:23 01:04:47:01 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* TO CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* SOURCE FILE: TC R1 V6 TEMP2 ST BG.WAV
019  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:04:46:23 01:04:46:23 
019  TC_R1_V6 A12   D    002 00:00:00:00 00:00:00:00 01:04:46:23 01:04:47:01 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* TO CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
020  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:04:47:00 01:05:47:12 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
021  TC_R1_V6 A11   C        00:00:00:00 00:00:00:00 01:04:47:01 01:05:47:12 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* SOURCE FILE: TC R1 V6 TEMP2 ST BG.WAV
022  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:04:47:01 01:05:47:12 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
023  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:05:47:12 01:06:08:06 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
024  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:05:47:12 01:07:27:09 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
025  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:05:47:12 01:07:27:09 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
026  TC_R1_V6 A11   C        00:00:00:00 00:00:00:00 01:05:47:12 01:10:21:10 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* SOURCE FILE: TC R1 V6 TEMP2 ST BG.WAV
027  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:06:08:06 01:07:27:01 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* A12 VOL =  +3.0 DB  PAN L100 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
028  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:07:27:09 01:07:27:09 
028  TC_R1_V1 A     D    002 00:00:00:00 00:00:00:00 01:07:27:09 01:07:27:11 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* TO CLIP NAME:  TC R1 V1.2 TEMP1 DX M.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
029  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:07:27:09 01:07:27:09 
029  TC_R1_V1 A7    D    002 00:00:00:00 00:00:00:00 01:07:27:09 01:07:27:11 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* TO CLIP NAME:  TC R1 V1.2 TEMP1 FX ST.WAV 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* PATCH TC_R1_V3:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
030  TC_R1_V1 A     C        00:00:00:00 00:00:00:00 01:07:27:11 01:07:36:22 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 DX M.WAV 
* SOURCE FILE: TC R1 V1.2 TEMP1 DX M.WAV
031  TC_R1_V1 A7    C        00:00:00:00 00:00:00:00 01:07:27:11 01:07:36:22 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 FX ST.WAV 
* PATCH TC_R1_V3:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V1.2 TEMP1 FX ST.WAV
032  TC_R1_V1 A     C        00:00:00:00 00:00:00:00 01:07:36:22 01:07:36:22 
032  TC_R1_V1 A     D    002 00:00:00:00 00:00:00:00 01:07:36:22 01:07:37:00 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 DX M.WAV 
* TO CLIP NAME:  TC R1 V1.2 TEMP1 DX M.WAV 
* SOURCE FILE: TC R1 V1.2 TEMP1 DX M.WAV
033  TC_R1_V1 A7    C        00:00:00:00 00:00:00:00 01:07:36:22 01:07:36:22 
033  TC_R1_V1 A7    D    002 00:00:00:00 00:00:00:00 01:07:36:22 01:07:37:00 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 FX ST.WAV 
* TO CLIP NAME:  TC R1 V1.2 TEMP1 FX ST.WAV 
* PATCH TC_R1_V3:  FROM SOURCE 2 TO RECORD 7 
* PATCH TC_R1_V3:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V1.2 TEMP1 FX ST.WAV
034  TC_R1_V1 A     C        00:00:00:00 00:00:00:00 01:07:37:00 01:07:49:01 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 DX M.WAV 
* SOURCE FILE: TC R1 V1.2 TEMP1 DX M.WAV
035  TC_R1_V1 A7    C        00:00:00:00 00:00:00:00 01:07:37:00 01:07:49:01 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 FX ST.WAV 
* PATCH TC_R1_V3:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V1.2 TEMP1 FX ST.WAV
036  TC_R1_V1 A     C        00:00:00:00 00:00:00:00 01:07:49:01 01:07:49:01 
036  TC_R1_V1 A     D    002 00:00:00:00 00:00:00:00 01:07:49:01 01:07:49:03 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 DX M.WAV 
* TO CLIP NAME:  TC R1 V1.2 TEMP1 DX M.WAV 
* SOURCE FILE: TC R1 V1.2 TEMP1 DX M.WAV
037  TC_R1_V1 A7    C        00:00:00:00 00:00:00:00 01:07:49:01 01:07:49:01 
037  TC_R1_V1 A7    D    002 00:00:00:00 00:00:00:00 01:07:49:01 01:07:49:03 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 FX ST.WAV 
* TO CLIP NAME:  TC R1 V1.2 TEMP1 FX ST.WAV 
* PATCH TC_R1_V3:  FROM SOURCE 2 TO RECORD 7 
* PATCH TC_R1_V3:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V1.2 TEMP1 FX ST.WAV
038  TC_R1_V1 A     C        00:00:00:00 00:00:00:00 01:07:49:03 01:08:56:09 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 DX M.WAV 
* SOURCE FILE: TC R1 V1.2 TEMP1 DX M.WAV
039  TC_R1_V1 A7    C        00:00:00:00 00:00:00:00 01:07:49:03 01:08:56:09 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 FX ST.WAV 
* PATCH TC_R1_V3:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V1.2 TEMP1 FX ST.WAV
040     BL    A12   C        00:00:00:00 00:00:00:00 01:08:56:00 01:08:56:00 
040  TC_R1_V6 A12   D    002 00:00:00:00 00:00:00:00 01:08:56:00 01:08:56:02 
* TO CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: (NULL)
041  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:08:56:02 01:10:21:10 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
042  TC_R1_V1 A     C        00:00:00:00 00:00:00:00 01:08:56:09 01:08:56:09 
042  TC_R1_V6 A     D    002 00:00:00:00 00:00:00:00 01:08:56:09 01:08:56:11 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 DX M.WAV 
* TO CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V1.2 TEMP1 DX M.WAV
043  TC_R1_V1 A7    C        00:00:00:00 00:00:00:00 01:08:56:09 01:08:56:09 
043  TC_R1_V6 A7    D    002 00:00:00:00 00:00:00:00 01:08:56:09 01:08:56:11 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 FX ST.WAV 
* TO CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* PATCH TC_R1_V3:  FROM SOURCE 2 TO RECORD 7 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V1.2 TEMP1 FX ST.WAV
044  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:08:56:11 01:10:21:10 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
045  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:08:56:11 01:10:21:10 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
046  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:10:21:10 01:11:34:01 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
047  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:10:21:10 01:11:54:07 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
048  TC_R1_V6 A11   C        00:00:00:00 00:00:00:00 01:10:21:10 01:11:54:07 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* SOURCE FILE: TC R1 V6 TEMP2 ST BG.WAV
049  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:10:21:10 01:11:54:07 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
050  LINE_02_ A5    C        00:00:00:00 00:00:00:00 01:11:36:10 01:11:37:10 
* FROM CLIP NAME:  LINE 02_08.L.WAV 
* PATCH LINE_02_:  FROM SOURCE 2 TO RECORD 5 
* SOURCE FILE: LINE 02_08.L.WAV
051  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:11:36:23 01:11:46:01 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
052  TC_R1_V6 A2    C        00:00:00:00 00:00:00:00 01:11:46:01 01:11:47:08 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* A2 VOL =  -3.0 DB  PAN L100 
* PATCH TC_R1_V6:  FROM SOURCE 1 TO RECORD 2 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
053  TC_R1_V6 A2    C        00:00:00:00 00:00:00:00 01:11:47:08 01:11:47:20 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* A2 VOL =  -3.0 DB  PAN L100 
* PATCH TC_R1_V6:  FROM SOURCE 1 TO RECORD 2 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
054  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:11:47:19 01:11:48:07 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* A1 VOL =  -3.0 DB  PAN R100 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
055  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:11:48:07 01:11:54:07 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
056  TC_R1_V6 A11   C        00:00:00:00 00:00:00:00 01:11:54:07 01:12:09:17 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* SOURCE FILE: TC R1 V6 TEMP2 ST BG.WAV
057  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:11:54:07 01:12:10:04 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
058  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:11:54:07 01:12:12:10 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
059  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:11:54:07 01:12:17:01 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
060     BL    A10   C        00:00:00:00 00:00:00:00 01:12:09:16 01:12:09:16 
060  TC_R1_V1 A10   D    002 00:00:00:00 00:00:00:00 01:12:09:16 01:12:09:18 
* TO CLIP NAME:  TC R1 V1.2 TEMP1 BG ST.WAV 
* A10 VOL =  +6.0 DB  PAN L100 
* PATCH TC_R1_V1:  FROM SOURCE 2 TO RECORD 10 
* SOURCE FILE: (NULL)
061  TC_R1_V1 A10   C        00:00:00:00 00:00:00:00 01:12:09:18 01:12:26:22 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 BG ST.WAV 
* A10 VOL =  +6.0 DB  PAN L100 
* PATCH TC_R1_V1:  FROM SOURCE 2 TO RECORD 10 
* SOURCE FILE: TC R1 V1.2 TEMP1 BG ST.WAV
062  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:12:10:04 01:12:10:04 
062  TC_R1_V6 A     D    002 00:00:00:00 00:00:00:00 01:12:10:04 01:12:10:06 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* TO CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
063  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:12:10:06 01:12:10:22 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
064  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:12:10:22 01:12:10:22 
064  TC_R1_V6 A     D    002 00:00:00:00 00:00:00:00 01:12:10:22 01:12:11:00 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* TO CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
065  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:12:11:00 01:12:17:01 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
066  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:12:12:10 01:12:17:01 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
067  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:12:17:01 01:12:27:00 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
068  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:12:17:01 01:12:27:00 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
069  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:12:17:01 01:12:27:00 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
070  TC_R1_V1 A10   C        00:00:00:00 00:00:00:00 01:12:26:22 01:12:26:22 
070  TC_R1_V1 A10   D    004 00:00:00:00 00:00:00:00 01:12:26:22 01:12:27:02 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 BG ST.WAV 
* TO CLIP NAME:  TC R1 V1.2 TEMP1 BG ST.WAV 
* A10 VOL =  +6.0 DB  PAN L100 
* A10 VOL =  +6.0 DB  PAN L100 
* PATCH TC_R1_V1:  FROM SOURCE 2 TO RECORD 10 
* PATCH TC_R1_V1:  FROM SOURCE 2 TO RECORD 10 
* SOURCE FILE: TC R1 V1.2 TEMP1 BG ST.WAV
071  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:12:27:00 01:12:50:19 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
072  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:12:27:00 01:12:50:19 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
073  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:12:27:00 01:12:50:19 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
074  TC_R1_V1 A10   C        00:00:00:00 00:00:00:00 01:12:27:02 01:13:14:13 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 BG ST.WAV 
* A10 VOL =  +6.0 DB  PAN L100 
* PATCH TC_R1_V1:  FROM SOURCE 2 TO RECORD 10 
* SOURCE FILE: TC R1 V1.2 TEMP1 BG ST.WAV
075  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:12:50:19 01:13:00:09 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
076  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:12:50:19 01:13:00:09 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
077  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:12:50:19 01:13:00:18 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* A7 VOL =  +0.0 DB  PAN R100 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
078  SROY-12B A     C        17:03:33:22 17:03:40:16 01:13:00:09 01:13:07:03 
* FROM CLIP NAME:  20A-1A 
* SOURCE FILE: A079C004_170801_R0M8
079  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:13:00:09 01:13:12:00 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
080  TC_R1_V6 A8    C        00:00:00:00 00:00:00:00 01:13:04:23 01:13:07:22 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* A8 VOL =  -6.0 DB  PAN L100 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 8 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
081  SROY-12B A2    C        17:13:10:23 17:13:12:22 01:13:07:00 01:13:08:23 
* FROM CLIP NAME:  20A-2A 
* PATCH SROY-12B:  FROM SOURCE 1 TO RECORD 2 
* SOURCE FILE: A079C004_170801_R0M8
082  TC_R1_V6 A8    C        00:00:00:00 00:00:00:00 01:13:07:22 01:13:07:22 
082  TC_R1_V6 A8    D    380 00:00:00:00 00:00:00:00 01:13:07:22 01:13:23:18 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* TO CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* A8 VOL =  -6.0 DB  PAN L100 
* A8 VOL =  +0.0 DB  PAN L100 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 8 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 8 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV 
* REPAIR:  TRANSITION DURATION TRIMMED FROM 380 FRAMES DUE TO FORMAT LIMITS
083  SROY-12B A     C        17:03:42:07 17:03:43:11 01:13:08:18 01:13:09:22 
* FROM CLIP NAME:  20A-1A 
* SOURCE FILE: A079C004_170801_R0M8
084  SROY-12B A2    C        17:13:02:03 17:13:03:13 01:13:09:17 01:13:11:03 
* FROM CLIP NAME:  20A-2A 
* PATCH SROY-12B:  FROM SOURCE 1 TO RECORD 2 
* SOURCE FILE: A079C004_170801_R0M8
085  SROY-12B A2    C        17:13:03:13 17:13:03:13 01:13:11:03 01:13:11:03 
085  SROY-12B A2    D    002 17:13:10:22 17:13:11:00 01:13:11:03 01:13:11:05 
* FROM CLIP NAME:  20A-2A 
* TO CLIP NAME:  20A-2A 
* PATCH SROY-12B:  FROM SOURCE 1 TO RECORD 2 
* PATCH SROY-12B:  FROM SOURCE 1 TO RECORD 2 
* SOURCE FILE: A079C004_170801_R0M8
086  SROY-12B A2    C        17:13:11:00 17:13:12:05 01:13:11:05 01:13:12:10 
* FROM CLIP NAME:  20A-2A 
* PATCH SROY-12B:  FROM SOURCE 1 TO RECORD 2 
* SOURCE FILE: A079C004_170801_R0M8
087  SROY-12B A     C        17:03:45:12 17:03:46:07 01:13:11:23 01:13:12:18 
* FROM CLIP NAME:  20A-1A 
* SOURCE FILE: A079C004_170801_R0M8
088  SROY-12B A2    C        17:13:09:23 17:13:11:01 01:13:12:15 01:13:13:17 
* FROM CLIP NAME:  20A-2A 
* PATCH SROY-12B:  FROM SOURCE 1 TO RECORD 2 
* SOURCE FILE: A079C004_170801_R0M8
089  SROY-12B A     C        17:03:47:02 17:03:48:08 01:13:13:13 01:13:14:19 
* FROM CLIP NAME:  20A-1A 
* SOURCE FILE: A079C004_170801_R0M8
090  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:13:13:19 01:13:19:19 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
091  TC_R1_V1 A10   C        00:00:00:00 00:00:00:00 01:13:14:13 01:13:14:13 
091  TC_R1_V1 A10   D    010 00:00:00:00 00:00:00:00 01:13:14:13 01:13:14:23 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 BG ST.WAV 
* TO CLIP NAME:  TC R1 V1.2 TEMP1 BG ST.WAV 
* A10 VOL =  +6.0 DB  PAN L100 
* A10 VOL =  +6.0 DB  PAN L100 
* PATCH TC_R1_V1:  FROM SOURCE 2 TO RECORD 10 
* PATCH TC_R1_V1:  FROM SOURCE 2 TO RECORD 10 
* SOURCE FILE: TC R1 V1.2 TEMP1 BG ST.WAV
092  SROY-12B A2    C        17:13:09:23 17:13:12:07 01:13:14:19 01:13:17:03 
* FROM CLIP NAME:  20A-2A 
* PATCH SROY-12B:  FROM SOURCE 1 TO RECORD 2 
* SOURCE FILE: A079C004_170801_R0M8
093  TC_R1_V1 A10   C        00:00:00:00 00:00:00:00 01:13:14:23 01:13:55:05 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 BG ST.WAV 
* A10 VOL =  +6.0 DB  PAN L100 
* PATCH TC_R1_V1:  FROM SOURCE 2 TO RECORD 10 
* SOURCE FILE: TC R1 V1.2 TEMP1 BG ST.WAV
094  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:13:17:03 01:13:24:00 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
095  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:13:19:19 01:13:19:19 
095  TC_R1_V6 A12   D    020 00:00:00:00 00:00:00:00 01:13:19:19 01:13:20:15 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* TO CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
096  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:13:20:15 01:14:04:18 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
097  TC_R1_V6 A8    C        00:00:00:00 00:00:00:00 01:13:23:18 01:13:23:20 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* A8 VOL =  +0.0 DB  PAN L100 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 8 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
098  TC_R1_V6 A8    C        00:00:00:00 00:00:00:00 01:13:23:20 01:13:38:00 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* A8 VOL =  +0.0 DB  PAN L100 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 8 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
099  SROY-12B A2    C        17:13:21:08 17:13:27:18 01:13:24:00 01:13:30:10 
* FROM CLIP NAME:  20A-2A 
* PATCH SROY-12B:  FROM SOURCE 1 TO RECORD 2 
* SOURCE FILE: A079C004_170801_R0M8
100  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:13:29:10 01:14:04:18 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
101  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:13:42:04 01:13:53:15 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* A7 VOL =  +0.0 DB  PAN R100 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
102  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:13:53:15 01:13:53:15 
102  TC_R1_V6 A7    D    002 00:00:00:00 00:00:00:00 01:13:53:15 01:13:53:17 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* TO CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* A7 VOL =  +0.0 DB  PAN R100 
* A7 VOL =  +2.0 DB  PAN R100 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
103  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:13:53:17 01:14:04:18 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* A7 VOL =  +2.0 DB  PAN R100 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
104  TC_R1_V1 A10   C        00:00:00:00 00:00:00:00 01:13:55:05 01:13:55:05 
104  TC_R1_V1 A10   D    008 00:00:00:00 00:00:00:00 01:13:55:05 01:13:55:13 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 BG ST.WAV 
* TO CLIP NAME:  TC R1 V1.2 TEMP1 BG ST.WAV 
* A10 VOL =  +6.0 DB  PAN L100 
* PATCH TC_R1_V1:  FROM SOURCE 2 TO RECORD 10 
* PATCH TC_R1_V1:  FROM SOURCE 2 TO RECORD 10 
* SOURCE FILE: TC R1 V1.2 TEMP1 BG ST.WAV
105  TC_R1_V1 A10   C        00:00:00:00 00:00:00:00 01:13:55:13 01:14:04:17 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 BG ST.WAV 
* PATCH TC_R1_V1:  FROM SOURCE 2 TO RECORD 10 
* SOURCE FILE: TC R1 V1.2 TEMP1 BG ST.WAV
106     BL    A11   C        00:00:00:00 00:00:00:00 01:14:00:21 01:14:00:21 
106  TC_R1_V6 A11   D    008 00:00:00:00 00:00:00:00 01:14:00:21 01:14:01:05 
* TO CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* SOURCE FILE: (NULL)
107  TC_R1_V6 A11   C        00:00:00:00 00:00:00:00 01:14:01:05 01:14:04:18 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* SOURCE FILE: TC R1 V6 TEMP2 ST BG.WAV
108  TC_R1_V1 A10   C        00:00:00:00 00:00:00:00 01:14:04:17 01:14:04:17 
108     BL    A10   D    001 00:00:00:00 00:00:00:01 01:14:04:17 01:14:04:18 
* FROM CLIP NAME:  TC R1 V1.2 TEMP1 BG ST.WAV 
* PATCH TC_R1_V1:  FROM SOURCE 2 TO RECORD 10 
* SOURCE FILE: TC R1 V1.2 TEMP1 BG ST.WAV
109  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:14:04:18 01:14:08:01 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* A7 VOL =  +2.0 DB  PAN R100 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
110  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:14:04:18 01:14:12:01 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
111  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:14:04:18 01:14:13:07 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
112  TC_R1_V6 A11   C        00:00:00:00 00:00:00:00 01:14:04:18 01:14:13:07 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* SOURCE FILE: TC R1 V6 TEMP2 ST BG.WAV
113  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:14:08:01 01:14:08:01 
113  TC_R1_V6 A7    D    002 00:00:00:00 00:00:00:00 01:14:08:01 01:14:08:03 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* TO CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* A7 VOL =  +2.0 DB  PAN R100 
* A7 VOL =  +0.0 DB  PAN R100 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
114  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:14:08:03 01:14:13:07 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* A7 VOL =  +0.0 DB  PAN R100 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
115  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:14:12:01 01:14:12:01 
115  TC_R1_V6 A12   D    090 00:00:00:00 00:00:00:00 01:14:12:01 01:14:15:19 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* TO CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
116  TC_R1_V6 A     C        00:00:00:00 00:00:00:00 01:14:13:07 01:16:55:17 
* FROM CLIP NAME:  TC R1 V6 TEMP2 M DX.WAV 
* SOURCE FILE: TC R1 V6 TEMP2 M DX.WAV
117  TC_R1_V6 A7    C        00:00:00:00 00:00:00:00 01:14:13:07 01:16:55:17 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST FX.WAV 
* PATCH TC_R1_V5:  FROM SOURCE 2 TO RECORD 7 
* SOURCE FILE: TC R1 V6 TEMP2 ST FX.WAV
118  TC_R1_V6 A11   C        00:00:00:00 00:00:00:00 01:14:13:07 01:16:55:17 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST BG.WAV 
* PATCH TC_R1_V4:  FROM SOURCE 2 TO RECORD 11 
* SOURCE FILE: TC R1 V6 TEMP2 ST BG.WAV
119  TC_R1_V6 A12   C        00:00:00:00 00:00:00:00 01:14:15:19 01:16:55:17 
* FROM CLIP NAME:  TC R1 V6 TEMP2 ST MX.WAV 
* PATCH TC_R1_V7:  FROM SOURCE 2 TO RECORD 12 
* SOURCE FILE: TC R1 V6 TEMP2 ST MX.WAV
120  OY_TAIL_ A2    C        00:00:00:00 00:00:00:00 01:16:51:16 01:16:55:17 
* FROM CLIP NAME:  TAIL LEADER STEREO 
* PATCH OY_TAIL_:  FROM SOURCE 1 TO RECORD 2 
* SOURCE FILE: OY_TAIL LEADER.MOV
*
* ============================================================
* Marker Metadata
* ------------------------------------------------------------
* 
* Sequence name: DC7 R1_v8.2
* Number  Color   Marker Name              Start TC    End TC      Duration    Track  Part        Comment
*      1  White   WBROGO                   01:02:12:00                         V1                 002_020 - Phone Screen - CU
*      2  White   WBROGO                   01:02:33:08                         V1                 004_010 - Remove Coke Logo
*      3  White   WBROGO                   01:03:00:16                         V1                 004_020 - Remove Logo - Equal
*      4  White   WBROGO                   01:03:48:03                         V1                 004_015 - Remove Jack Jerk / line before he says "what"
*      5  White   WBROGO                   01:03:55:08                         V1                 004_030 - Split screen - Comp other hand into shot
*      6  White   WBROGO                   01:04:21:13                         V1                 004_040 - Split Screen - Simple
*      7  White   WBROGO                   01:04:32:19                         V1                 008_010 - Phone Screen - CU
*      8  White   WBROGO                   01:05:34:10                         V1                 008_015 - Phone Screen - Distant
*      9  White   WBROGO                   01:05:44:00                         V1                 008_020 - Phone Screen - CU
*     10  White   WBROGO                   01:06:00:01                         V1                 011_010 - Phone Screen - Distant
*     11  White   WBROGO                   01:08:16:06                         V1                 016_005 - Add family photos on wall behind jack to match later when sees Ash dead
*     12  White   WBROGO                   01:08:30:23                         V1                 016_007 - Add family photos on wall behind jack to match later when sees Ash dead
*     13  White   WBROGO                   01:08:36:16                         V1                 016_010 - Make dog look less fake / reverse to extend timing
*     14  Red     SCOTT_H                  01:08:57:12                         V1                 Color Note: Vignette or window to focus our eye into the mirror to see the dead body
*     15  White   WBROGO                   01:09:43:14                         V1                 016_020 - Add family photos behind Jack
*     16  White   WBROGO                   01:11:16:10                         V1                 018_020 - Add headstones / Stabalize
*     17  White   WBROGO                   01:12:39:09                         V1                 020_015 - Phone Screen - CU - Comp video with push in
*     18  Red     SCOTT_H                  01:12:58:19                         V1                 NEW VFX SHOT
*     19  White   SCOTT_H                  01:12:59:01                         V1                 VFX shot morph for performance speed.
*     20  White   WBROGO                   01:13:19:22                         V1                 020_020 - Phone Screen - CU
*     21  White   WBROGO                   01:13:37:21                         V1                 020_030 - Phone Screen - CU
*     22  White   WBROGO                   01:13:52:12                         V1                 020_040 - Phone Screen - CU - Match thumb to click
*     23  White   WBROGO                   01:14:22:05                         V1                 021_010 - remove boom reflection / clean up light when actor leans back
*     24  White   WBROGO                   01:15:01:14                         V1                 024_010 - Remove camera operator from mirror / Phone Screen / Add picture frames on wall to match Sc 16 when Jack sees Ash dead
*     25  White   WBROGO                   01:15:24:17                         V1                 024_020 - Phone Screen CU
*     26  Yellow  SCOTT_H                  01:08:26:16                         V2                 Speed change. 
*
*     27  White   WBROGO                   01:09:59:14                         V2                 016_030 - Add family photos on wall
*     28  White   WBROGO                   01:11:40:22                         V2                 018_030 - Add headstones
*     29  Red     SCOTT_H                  01:11:41:11                         V2                 Moved retimed
*     30  Red     SCOTT_H                  01:09:10:13                         A6                 KEEP IN TIME LINE. ADR OF DAVID for his moans etc...to keep in timeline in case needed by JE in the mix
>>> SOURCE SROY-12B SROY-12B 060a2b340101010101010f00-13-00-00-00-{00000511-6f6e-53f5-060e2b347f7f2a80} 
* SOURCE FILE: A079C004_170801_R0M8